*********************************************************************************
                    GK5CQ7Z&GK7CP7S&GK5CP0Z EC RELEASE NOTE

*********************************************************************************
---------------------------------------------------------------------------------
2019/01/16    		     EC Version 1.03.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ10.309   				      Checksum: 00d9d14dh
File name: GKxCPQ10.329   				      Checksum: 00d9d356h
File name: GKxCPQ10.339					      Checksum: 00d9b190h
1.Decrease KB scan speed to 24ms and remove break debounce workaround.(Improve KB signal quality)
2.Fix usb KB can't use in Dos mode.
3.Add EC common source code--20181222_Make AdapterI more accurate

Note:
     Release Formal version "1.03.09" for Standard
     Release sub version    "1.03.29" for XMG
     Release sub version    "1.03.39" for Haier
---------------------------------------------------------------------------------
2019/01/07    		     EC Version 1.02.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ10.209   				      Checksum: 00d94ddah
File name: GKxCPQ10.229   				      Checksum: 00d94fe3h
File name: GKxCPQ10.239					      Checksum: 00d94c0ch
1.Fix flash fail issue.
2.Send D state after 60 seconds delay of get os type during warmboot and coldboot.
Note:
     Release Formal version "1.02.09" for Standard
     Release sub version    "1.02.29" for XMG
     Release sub version    "1.02.39" for Haier
---------------------------------------------------------------------------------
2019/01/02    		     EC Version 1.01.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ10.109   				      Checksum: 00d95ce8h
File name: GKxCPQ10.129   				      Checksum: 00d95ef1h
File name: GKxCPQ10.139					      Checksum: 00d968e5h
1.Add WA for FnF6/F7 can't adjust KB BL by smbus.
2.Add WA for EC ROM sequence doesn't meet spec.
3.Add clear KB buffer before scan.

Note:
     Release Formal version "1.01.09" for Standard
     Release sub version    "1.01.29" for XMG
     Release sub version    "1.01.39" for Haier
---------------------------------------------------------------------------------
2018/12/24    		     EC Version 1.00.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ10.009   				      Checksum: 00d97a93h
File name: GKxCPQ10.029   				      Checksum: 00d97c9ch
File name: GKxCPQ10.039					      Checksum: 00d962afh
1.Delay 500ms to turn on PCH_PWROK in S3 resume sequence-for type-C detect issue.

Note:
     Release Formal version "1.00.09" for Standard
     Release sub version    "1.00.29" for XMG
     Release sub version    "1.00.39" for Haier
---------------------------------------------------------------------------------
2018/12/21    		     EC Version 0.15.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.509   				      Checksum: 00d9865fh
File name: GKxCPQ01.539   				      Checksum: 00d95e73h
File name: GKxCPQ01.529					      Checksum: 00d98868h
1.Update 0Z/7Z/0S Power Management table.
2.Add solution for screen blink when resume from S3.(Follow GK7CN5R)
3.Set power limit by Q70.
4.Add WA for auto enter CMOS setup.
5.Modify 7S  fan table.
	file:GK7CP7S_B_phase_Thermal_Fan Speed Control Table_20181218.pdf
Note:
     Release Formal version "0.15.09" for Standard
     Release sub version    "0.15.29" for XMG
     Release sub version    "0.15.39" for Haier
---------------------------------------------------------------------------------
2018/12/11    		     EC Version 0.14.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.409   				      Checksum: 00d9c1aeh
1.Set power limit by PECI.
2.Update 7S/7Z/8S Power Management table according Power Management Template v1.03 -Smart APC 20181210.xlsx
***Please make sure BIOS support Power Limit setting by  EC self(remove Q70).
---------------------------------------------------------------------------------
2018/12/10    		     EC Version 0.13.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.309   				      Checksum: 00d88446h
1.Modify  power management table(Rev 1.03).
2.Pull rsmrst after power off when protectshudown and override shutdown
3.Add clear keyboard buffer during power off and powen on.
4.Add  fan run 80% duty when battery temperature over 57 degrees in non os.
5.Add ITE keyboard OBF solution.
6.Add protect shutdown item--battery discharge 6% shutdown in non OS.
7.Set DGPU_PWR_ON(GPI1) low and prochot active durning DC mode power off.
8.Fn+F4 switch lock 10S
9.Fix ZeroI calibration incorrect issue.
10.Delay PCH_PWROK 500ms in power_on sequence for type-C detect issue.
11.Modify 7Z/0Z/0S  fan table.
	file:GK7CP0S_B_phase_Thermal_Fan Speed Control Table_20181120.pdf
	file:GK5CQ7Z_B_phase_Thermal_Fan Speed Control Table_20181206.pdf
---------------------------------------------------------------------------------
2018/11/28    		     EC Version 0.12.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.209   				      Checksum: 00db638ah
1.Modify Power management table.
2.Pull prochot and GPIO12 pin in DC and non OS mode .
3.Fix show numlock OSD when resume from DC mode S4.
4.Add mode indicator LED.
5.Add EC common source code--20181123_Send_DS_SciEvent@PwOn
6.Add EC common source code--20181127_AC in and Battery not exist still need run smart APC.
7.Modify 7S  fan table.
	file:GK7CP7S_B_phase_Thermal_Fan Speed Control Table_20181120a_internal
---------------------------------------------------------------------------------
2018/11/9    		     EC Version 0.11.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.109   				      Checksum: 00db7a12h
1.Add ID Pin for GK7CQ8S
2.Change BAT_I ratio follow HW circurt value (0.1724V/1A).
3.Add EC common source code--20181107_MPS Fw Info  move to 07xx
4.Support 2.5mohm AC R-sense.  
5.Support Power Management Template v1.02.
6.Modify charger battery Depletion Threshold equal to lowest level(59.19%)
7.Set 180W power mangement setting as default.
8.Modify 7S  fan table.
	file:GK7CP7S_A_phase_Thermal_Fan Speed Control Table_20181029.pdf
---------------------------------------------------------------------------------
2018/10/26    		     EC Version 0.10.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ01.009   				      Checksum: 00dc4864h
1.Modify GPIO for B Phase.
2.Add EC common source code--20181025_Support Smart APC + 9.3A BAT_I
3.Add EC common source code--20181023_Modify ZeroI calibration algorithm.
4.Add EC common source code--20181019_inital WA3081 timer at early power on sequence.
5.Add 7S 7Z B phase fan table.
	file:GK7CP7S_A_phase_Thermal_Fan Speed Control Table_20181015.pdf
	file:GK5CQ7Z_A_phase_Thermal_Fan Speed Control Table_20181018.pdf
** B phase EC from this version 
---------------------------------------------------------------------------------
2018/10/17    		     EC Version 0.03.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ00.309   				      Checksum: 00dddb2dh
1.Fix AC in auto power on while RTC power lose.
2.Add 7Z fan table according GK5CQ7Z_A_phase_Thermal_Fan Speed Control Table_20181015.pdf
3.Add EC common source code--20181005_2nd Generation ME Keyboard_Support PCBA v1.4(Update09 for add break-debounce function)
4.Add EC common source code--20181002_for GamingCenter show the lowest and highest CPU temperature of fan on .
--------------------------------------------------------------------------------
2018/09/27    		     EC Version 0.02.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ00.209   				      Checksum: 00de2c70h
1.Add HW ID (GPC6)for GK5CP0Z
2.EC code compatiable with ITE5571(Based on ITE5571 1.04.110M.zip file)
3.Add MPS IC fw read.
4.Modify 230W AC performance. 
---------------------------------------------------------------------------------
2018/09/03    		     EC Version 0.01.09		      Owner: Qin.Zong
---------------------------------------------------------------------------------
File name: GKxCPQ_00.109   				      Checksum: 00e1ac57h
1.First release for A phase ,based on GK5CN EC version 1.29.09.